HRSA 2024 Uniform Data System (UDS) Patient Level Submission (PLS) (UDS+) FHIR IG
2.0.0 - STU2 Release 1 - Standard for Trial-Use

Publication Build: This will be filled in by the publication tooling

## CapabilityStatement: Uds Plus Data Receiver CapabilityStatement

Official URL: http://fhir.org/guides/hrsa/uds-plus/CapabilityStatement/uds-plus-data-receiver-server | Version: 2.0.0
Standards status: Trial-use | Maturity Level: 2 | Computable Name: UdsPlusDataReceiverServer

This is a CapabilityStatement that defines the expected capabilities of the Data Receiver actor as a Server.

Raw OpenAPI-Swagger Definition file | Download

## Data Receiver

(Requirements Definition Capability Statement)

Canonical URL: http://fhir.org/guides/hrsa/uds-plus/CapabilityStatement/uds-plus-data-receiver-server

Published by: HL7 International - Public Health Work Group

This is a CapabilityStatement that defines the expected capabilities of the Data Receiver Server actor.

## General

FHIR Version: | 4.0.1
Supported formats: | json

## REST behavior

The primary focus of the Data Receiver as a Server is to receive the manifest which contains the links to the UDS+ data that has been extracted by the health center and is being made available to HRSA.

Security:

Implementations must meet the general security requirements documented in FHIR Security guidance.

In addition the Data Receiver actor needs to meet the security requirements as outlined in the SMART on FHIR Backend Services Authorization

### FHIR Operations summary

The following FHIR operations SHALL be supported by the Data Source.

- UDS+ Import Operation
- Status Polling using Content-Location received for Bulk Data Import as part of the Content-Location HTTP Header