HRSA 2024 Uniform Data System (UDS) Patient Level Submission (PLS) (UDS+) FHIR IG
2.0.0 - STU2 Release 1 - Standard for Trial-Use

Publication Build: This will be filled in by the publication tooling

## Resource Profile: UDSPlusLocation - Mappings

Page standards status: Trial-use | Maturity Level: 2

Mappings for the uds-plus-location resource profile.

### Mappings for RIM Mapping (http://hl7.org/v3)

UDSPlusLocation
Location | Entity. Role, or Act, .Role[classCode=SDLC]
text | Act.text?
contained | N/A
extension | N/A
modifierExtension | N/A
identifier | .id
status | .statusCode
operationalStatus | n/a
name | .name
alias | .name
description | .playingEntity[classCode=PLC determinerCode=INSTANCE].desc
mode | .playingEntity[classCode=PLC].determinerCode
type | .code
telecom | .telecom
address | .addr
id | n/a
extension | n/a
use | unique(./use)
type | unique(./use)
text | ./formatted
line | AD.part[parttype = AL]
city | AD.part[parttype = CTY]
district | AD.part[parttype = CNT | CPA]
state | AD.part[parttype = STA]
postalCode | AD.part[parttype = ZIP]
country | AD.part[parttype = CNT]
period | ./usablePeriod[type="IVL<TS>"]
physicalType | .playingEntity [classCode=PLC].code
position | .playingEntity [classCode=PLC determinerCode=INSTANCE].positionText
id | n/a
extension | n/a
modifierExtension | N/A
longitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
latitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
altitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
managingOrganization | .scopingEntity[classCode=ORG determinerKind=INSTANCE]
partOf | .inboundLink[typeCode=PART].source[classCode=SDLC]
hoursOfOperation | .effectiveTime
id | n/a
extension | n/a
modifierExtension | N/A
daysOfWeek | .effectiveTime
allDay | .effectiveTime
openingTime | .effectiveTime
closingTime | .effectiveTime
availabilityExceptions | n/a
endpoint | n/a

### Mappings for FiveWs Pattern Mapping (http://hl7.org/fhir/fivews)

UDSPlusLocation
Location |
identifier | FiveWs.identifier
status | FiveWs.status
operationalStatus | FiveWs.status
mode | FiveWs.class
type | FiveWs.class
physicalType | FiveWs.class